**SECTION 09 54 21**

**METAL PAN CEILINGS**

**METALWORKS SECURELOCK PLUS**

# Part 1 - General

## 1.1 RELATED DOCUMENTS

A. Section Includes

 Drawings and general conditions of Contract, including General and Supplementary Conditions and Divisions-1 Specification sections apply to work of this section.

## 1.2 SUMMARY

A. Section Includes

 1. Acoustical metal ceiling panels

 2. Exposed grid suspension system

 3. Wire hangers, fasteners, main runners, cross tees, and wall angle moldings

 4. Perimeter Trim

B. Related Sections:

 1. Section 09 51 33.13 Acoustical Snap in Metal Pan Ceiling

 2. Section 09 20 00 (09250) - Plaster and Gypsum Board

 3. Section 09 51 13 (09500) - Acoustical Fabric-Faced Panel Ceilings

 4. Section 09 53 00 (09500) - Acoustical Ceiling Suspension Assemblies

 5. Section 09 54 00 Specialty Ceilings

 6. Divisions 23 - HVAC Air Distribution

 7. Division 26 - Electrical

C. Alternates

 1. Prior Approval: Unless otherwise provided for in the Contract documents, proposed product substitutions may be submitted no later than TEN (10) working days prior to the date established for receipt of bids. Acceptability of a proposed substitution is contingent upon the Architect's review of the proposal for acceptability and approved products will be set forth by the Addenda. If included in a Bid are substitute products that have not been approved by Addenda, the specified products shall be provided without additional compensation.

 2. Submittals that do not provide adequate data for the product evaluation will not be considered. The proposed substitution must meet all requirements of this section, including but not necessarily limited to, the following: Single source materials suppliers (if specified in Section 1.5); Underwriters' Laboratories Classified Acoustical performance; Panel design, size, composition, color, and finish; Suspension system component profiles and sizes; Compliance with the referenced standards.

## 1.3 REFERENCES

## A. American Society for Testing and Materials (ASTM):

1. ASTM A 1008 Standard Specification for Steel, Sheet, Cold Rolled, Carbon, Structural, High-Strength Low-Alloy and High-Strength Low-Alloy with Improved Formability

2. ASTM A 641 Standard Specification for Zinc-Coated (Galvanized) Carbon Steel Wire

3. ASTM A 653 Standard Specification for Steel Sheet, Zinc-Coated (Galvanized) by the Hot-Dip Process

4. ASTM C 423 Sound Absorption and Sound Absorption Coefficients by the Reverberation Room Method

5. ASTM C 635 Standard Specification for Metal Suspension Systems for Acoustical Tile and Lay-in Panel Ceilings

6. ASTM C 636 Recommended Practice for Installation of Metal Ceiling Suspension Systems for Acoustical Tile and Lay-in Panels

7. ASTM D 3273 Standard Test Method for Resistance to Growth of Mold on the Surface of Interior Coatings in an Environmental Chamber

8. ASTM E 84 Standard Test Method for Surface Burning Characteristics of Building Materials

9. ASTM E 580 Installation of Metal Suspension Systems in Areas Requiring Moderate Seismic Restraint

10. ASTM E 1111 Standard Test Method for Measuring the Interzone Attenuation of Ceilings Systems

11. ASTM E 1414 Standard Test Method for Airborne Sound Attenuation Between Rooms Sharing a Common Ceiling Plenum

12. ASTM E 1264 Classification for Acoustical Ceiling Products

## B. International Building Code

## C. ASHRAE Standard 62 1 2004 Ventilation for Acceptable Indoor Air Quality

## D. NFPA 70 National Electrical Code

## E. ASCE 7 American Society of Civil Engineers, Minimum Design Loads for Buildings and Other Structures

## F. International Code Council-Evaluation Services - AC 156 Acceptance Criteria for Seismic Qualification Testing of Non-structural Components

## G. International Code Council-Evaluation Services Report - Seismic Engineer Report

 1. ESR 1308 - Armstrong Suspension Systems

## H. LEED - Leadership in Energy and Environmental Design is a set of rating systems for the design, construction, operation, and maintenance of green buildings.

## 1.4 SYSTEM DESCRIPTION

Continuous/Wall-to-Wall

## 1.5 SUBMITTALS

A. Product Data: Submit manufacturer's technical data for each type of acoustical ceiling unit and suspension system required.

B. Samples: Minimum 6-inch x 6-inch samples of specified acoustical panel; 8-inch-long samples of exposed wall molding and suspension system, including main runner and 4-foot cross tees.

C. Shop Drawings: Layout and details of acoustical ceilings show locations of items that are to be coordinated with or supported by the ceilings.

D. Certifications: Manufacturer's certifications that products comply with specified requirements, including laboratory reports showing compliance with specified tests and standards. For acoustical performance, each carton of material must carry an approved independent laboratory classification of NRC, CAC, and AC.

E. If the material supplied by the acoustical subcontractor does not have an Underwriter's Laboratory classification of acoustical performance on every carton, subcontractor shall be required to send material from every production run appearing on the job to an independent or NVLAP approved laboratory for testing, at the architect's or owner's discretion. All products not conforming to manufacturer's current published values must be removed, disposed of, and replaced with complying product at the expense of the Contractor performing the work.

## 1.6 QUALITY ASSURANCE

A. Single-Source Responsibility: Provide acoustical panel units and grid components by a single manufacturer.

B. Fire Performance Characteristics: Identify acoustical ceiling components with appropriate markings of applicable testing and inspecting organization.

a. Surface Burning Characteristics: ASTM E 84 and complying with ASTM E 1264 Classification.

C. Acoustic Panels: As with other architectural features located at the ceiling, may obstruct, or skew the planned fire sprinkler water distribution pattern through possibly delay or accelerate the activation of the sprinkler or fire detection systems by channeling heat from a fire either toward or away from the device. Designers and installers are advised to consult a fire protection engineer, NFPA 13, or their local codes for guidance where automatic fire detection and suppression systems are present.

D. Coordination of Work: Coordinate acoustical ceiling work with installers of related work including, but not limited to building insulation, gypsum board, light fixtures, mechanical systems, electrical systems, and sprinklers.

## 1.7 DELIVERY, STORAGE AND HANDLING

A. Deliver acoustical ceiling units to project site in original, unopened packages and store them in a fully enclosed space where they will be protected against damage from moisture, direct sunlight, surface contamination, and other causes.

B. Before installing acoustical ceiling units, permit them to reach room temperature and a stabilized moisture content.

C. Handle acoustical ceiling units carefully to avoid chipping edges or damaged units in any way.

## 1.8 PROJECT CONDITIONS

A. Space Enclosure:

Standard Ceilings: Do not install interior ceilings until space is enclosed and weatherproof; wet work in place is completed and nominally dry; work above ceilings is complete; and ambient conditions of temperature and humidity are continuously maintained at values near those intended for final occupancy. Building areas to receive ceilings shall be free of construction dust and debris.

## 1.9 LEED

A. Armstrong Metal Ceilings qualify for the following credits:

 a. Category - Material & Resources

 i. MR Credit 2.1, 2.2 - Construction Waste Management Divert 50% or 75% from disposal

 ii. MR Credit 4.1, 4.2 - Recycled Content

 iii. MR Credit 5.1, 5.2 - Regional Materials (dependent on location)

 LEED NC - 10% Extracted, Processed & Manufactured Regionally

 LEED CI - 20% Manufactured Regionally

 b. Category - Indoor Environmental Quality

 i. EQ Credit 4.1 to 4.6 - Low-Emitting Materials

 c. Category - Innovation and Design Process

 i. ID Credit - Acoustic Performance

## 1.10 WARRANTY

A. Acoustical Panel: Submit a written warranty executed by the manufacturer, agreeing to repair or replace panels that fail within the warranty period. Failures include, but are not limited to the following:

 1. Acoustical Panels: Sagging and warping

 2. Grid System: Rusting and manufacturer's defects.

B. Warranty Period:

 1. Acoustical Metal panels: One (1) year from date of substantial completion

 2. Grid: One (1) year from date of substantial completion

C. The Warranty shall not deprive the Owner of other rights the Owner may have under other provisions of the Contract Documents and will be in addition to and run concurrent with other warranties made by the Contractor under the requirements of the Contract Documents.

## 1.11 MAINTENANCE

A. Extra Materials: Deliver extra materials to Owner. Furnish extra materials described below that match products installed. Packaged with protective covering for storage and identified with appropriate labels.

 1. Acoustical Metal Ceiling Units: Furnish quality of full-size units equal to 5.0 percent of amount installed.

 2. Exposed Suspension System Components: Furnish quantity of each exposed suspension component equal to 2.0 percent of amount installed.

# PART 2 – PRODUCTS

Attention Design Professional: Please edit Part 2 based on your project needs. Select product attributes and acceptable product item (s) that fit with the requirements of your project. Delete all items from the specification that do not relate to your project needs. Please refer to the Armstrong website for additional ceilings, suspension systems, perimeter trim options, and accessories. The related guide specifications for each of these items are available on the Armstrong website.

## 2.1 MANUFACTURERS

A. Metal Ceiling Panels:

 1. Armstrong World Industries, Inc.

B. Suspension Systems:

 1. Armstrong World Industries, Inc.

## 2.2.1 ACOUSTICAL CEILING UNITS

## A. Acoustical Panels Type AMP

1. Acoustical Panels Type AMP-1:
 a. Surface Texture: Smooth
 b. Composition: Electrogalvanized (12) (14) (16) gauge galvanized steel with postproduction powder coated paint finish
 c. Color:

* + - 1. White (WH)
			2. Silver Grey (SG)\*
			3. Gun Metal (MY)\*
			\*Premium finish options

 d. Size: (12 inch) (18 inch) (24 inch) widths, up to 12 foot lengths
 e. Edge Profile: Screw In Concealed Locking (tested to withstand 960 – 3100 lbs. of force)
 f. Perforation Option: (Unperforated-P1) (Perforated-P5)
 g. Noise Reduction Coefficient( NRC): ASTM C 423; Classified with UL label on product carton, (unperforated - N/A), (perforated with optional fiberglass infill item #8200100 – 0.80)
 h. Ceiling Attenuation Class (CAC) : N/A
 i. Sabin: N/A
 j. Articulation Class (AC): N/A
 k. Flame Spread: ASTM E 1264; Class A (FM)
 l. Light Reflectance: ASTM E 1477; White Panel: Light Reflectance: (unperforated - 0.75)
 m. Dimensional Stability: Standard
 n. Acceptable Product: MetalWorks SecureLock Plus, \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_, as manufactured by Armstrong World Industries.

2. Panel Accessories:

1. 1” Fiberglass Infill Panel, Item# 8200T10
2. Access Door panel, Item# 5949

3. Suspension System:

1. Edge Moldings: Metal or stainless steel of types and profiles indicated or, if not indicated, manufacturer's standard moldings for edges and penetrations, including light fixtures, that fit type of edge detail and suspension system indicated.
2. Accessories:
	1. SecureLock Plus Hold Down Clips; Item# 5595
	2. C Channel; 14-gauge, Item# 5397WH
	3. Midspan Strut; Item# 5593WH
	4. Z Clips; 14-gauge, Item# 5599

PART 3 - EXECUTION

## 3.1 EXAMINATION

A. Do not proceed with installation until all wet work such as concrete, terrazzo, plastering and painting has been completed and thoroughly dried out, unless expressly permitted by manufacturer's printed recommendations. (Exception: HumiGuard Max Ceilings)

## 3.2 PREPARATION

A. Measure each ceiling area and establish layout of acoustical units to balance border widths at opposite edges of each ceiling. Avoid use of less than half width units at borders and comply with reflected ceiling plans. Coordinate panel layout with mechanical and electrical fixtures.

## 3.3 INSTALLATION

1. Install suspension system and panels in compliance with ASTM C636, with the authorities having jurisdiction, and in accordance with the manufacturer's installation instructions:
	1. MetalWorks SecureLock Plus Installation Instructions, LA-297583
	2. MetalWorks Cutting Instructions, LA-295518
2. Install wall moldings at intersection of suspended ceiling and vertical surfaces. Miter corners where wall moldings intersect or install corner caps.
3. Follow the instructions found in "MetalWorks SecureLock Plus Installation Instructions", LA-297583 for border treatment of the MetalWorks SecureLock Plus panels. The face of the suspension system rests directly on the molding or trim flange.
4. Installation consideration: For a 12- or 16-gauge plank system, the perimeter connection must support a 3000 lb. upward load applied anywhere along the panel edge within 3 inches of the perimeter channel.
5. Panels with certain product finishes or characteristics, e.g., Sequels™ are part of our MetalWorks™ FASTPeel ™ Panel which come standard with our easier-to-remove protective film

## 3.4 ADJUSTING AND CLEANING

A. Replace damaged and broken panels.

B. Clean exposed surfaces of ceilings panels, including trim, edge moldings, and suspension members. Comply with manufacturer's instructions for cleaning and touch up of minor finish damage. Remove and replace work that cannot be successfully cleaned and repaired to permanently eliminate evidence of damage.